

**Ecoflame 2 Electric Fire Range**



The Ecoflame 2 is a Landscape style, inset or wall mount fire featuring a realistic flame effect and Pebble fuel bed.

It is available with a Flat (illustrated) or Curved Black glass fascia (note Curved glass must be Partial inset fixing). It is supplied as standard 1.5KW output which, in addition to saving energy, makes it particularly suited to environments where pitches have limited power availability.

The heat outlet is at the bottom of the fire and blows outwards to allow low mounting to within 60mm of working sufaces. The heat outlet is also disguised by the drop down grill which allows access to the manual controls instead of the remote control handset.

The Ecoflame 2 is supplied as standard with thermostat control and remote control.

The product complies with the ECO Design Directive (EU) 2015/1188

|  |
| --- |
| **SPECIFICATION** |
| **Overall height:** | 619mm |
| **Overall width:** | 800mm |
| **Overall depth:** |  140mm (125mm inset Depth) |
| **Weight:** | 10Kg |
| **Wall opening: (minimum)** | 535mm High x 440mm Wide |
| **Heat output:** | 1.5 kW  |
| **Lead length** | 2 metres |
| **Remote control available (Y/N)** | Y – Standard |
| **ECO Directive Compliant (2015/1188)** | Y |
| **7 Day Timer** | Y |
| **Auto Open Window Detection** | Y |
| **Adaptive Start Control** | Y |

Widney Leisure Ltd

St Marys Road, Nuneaton, Warwickshire CV11 5AU UK

TEL: 02476 377550 FAX: 02476 388578